//NEWTONPF  Solves power flow using full Newton's method (power/polar)
//   [V, CONVERGED, I] = NEWTONPF(YBUS, SBUS, V0, REF, PV, PQ, MPOPT)
//
//   Solves for bus voltages using a full Newton-Raphson method, using nodal
//   power balance equations and polar coordinate representation of
//   voltages, given the following inputs:
//       YBUS  - full system admittance matrix (for all buses)
//       SBUS  - handle to function that returns the complex bus power
//               injection vector (for all buses), given the bus voltage
//               magnitude vector (for all buses)
//       V0    - initial vector of complex bus voltages
//       REF   - bus index of reference bus (voltage ang reference & gen slack)
//       PV    - vector of bus indices for PV buses
//       PQ    - vector of bus indices for PQ buses
//       MPOPT - (optional) MATPOWER option struct, used to set the
//               termination tolerance, maximum number of iterations, and
//               output options (see MPOPTION for details).
//
//   The bus voltage vector contains the set point for generator
//   (including ref bus) buses, and the reference angle of the swing
//   bus, as well as an initial guess for remaining magnitudes and
//   angles.
//
//   Returns the final complex voltages, a flag which indicates whether it
//   converged or not, and the number of iterations performed.
//
//   See also RUNPF, NEWTONPF_S_CART, NEWTONPF_I_POLAR, NEWTONPF_I_CART.

//   MATPOWER
//   Copyright (c) 1996-2019, Power Systems Engineering Research Center (PSERC)
//   by Ray Zimmerman, PSERC Cornell
//
//   This file is part of MATPOWER.
//   Covered by the 3-clause BSD License (see LICENSE file for details).
//   See https://matpower.org for more info.

fn newtonpf(Ybus, Sbus, V0, ref, pv, pq, mpopt) {
    // options
    tol         = get(mpopt, 0);
    max_it      = get(mpopt, 1);

    // initialize
    converged = 0;
    i = 0;
    V = V0;
    Va = angle(V);
    Vm = abs(V);
    
    npv = length(pv);
    npq = length(pq);
    j1 = 1;         j2 = npv;           // j1:j2 - V angle of pv buses
    j3 = j2 + 1;    j4 = j2 + npq;      // j3:j4 - V angle of pq buses
    j5 = j4 + 1;    j6 = j4 + npq;      // j5:j6 - V mag of pq buses

    // evaluate F(x0)
    mis = V .* conj(Ybus * V) - Sbus(Vm);
   ·
}